Order Information

|  |  |
| --- | --- |
| **S6600A-06 L3 Distribution Switch Series** | |
| **Chassis and power supply** | |
| S6600A-06 | S6600A-06   chassis, two control engine slots, 4+2 service slots, 2 switching engines slots, two fan slot, four   power slots. |
| **Control Engine** | |
| SM66A-MPUE | SM66A-MPUE   Control Engine, supporting active/standby backup function (one is mandatory,   1+1 redundancy is optional) |
| **Switching Engine** | |
| SM66A-SFUE | SM66A-SFUE Standard Switching Engine (one is   mandatory, 1+1 redundancy is optional) |
| SM66A-SFUF | SM66A-SFUE Enhanced Switching Engine (one is   mandatory, 1+1 redundancy is optional) |
| **Fan Modules** | |
| FAN-11A-01 | FAN-11A-01   Fan Module for S6600A-06 |
| **Power Modules** | |
| AD800-1D005M | AD800-1D005M,   800W AC power module |
| AD1600-1D005M | AD1600-1D005M,   1600W AC power module |
| **Service Modules (Standard L2&L3 Features)** | |
| SM66A-8QXGE-FC | 8-port 40G QSFP+ optical interface   (SM66A-SFUF is mandatory) |
| SM66A-32XGEF-FC | 32-port 10G SFP+ optical interface   (SM66A-SFUF is mandatory) |
| SM66A-16XGEF-FC | 16-port 10G SFP+ optical interface |
| SM66A-24GET24GEF4XF-FC | 24-port 1000M Base-T electric   interface, 24-port 1000M SFP optical interface,4-port 10G SFP+ optical   interface |
| SM66A-48GEF4XGEF-FC | 48-port 1000M SFP optical   interface,4-port 10G SFP+ optical interface |
| SM66A-48GET4XGEF-FC | 48-port 1000M Base-T electric   interface,4-port 10G SFP+ optical interface |