# Order Information

|  |
| --- |
| **S6600A-04 L3 Distribution Switch Series**  |
| **Chassis and power supply** |
| S6600A-04 | S6600A-04 chassis, two control engine slots, 4 service slots, one fan slot, two power slots. |
| **Control Engine** |
| SM66A-MPUD | SM66A-MPUD Control Engine, supporting active/standby backup function (one is mandatory, 1+1 redundancy is optional) |
| **Fan Modules** |
| FAN-05C-01B | FAN-05C-01B Fan Module for IS660-04 |
| **Power Modules** |
| AD500M-HS0F | AD500M-HS0F, 500W AC power module |
| **Service Modules (Standard L2&L3 Features)**  |
| SM66A-16XGEF-FB | 16-port 10G SFP+ optical interface |
| SM66A-24GET24GEF4XF-FB | 24-port 1000M Base-T electric interface, 24-port 1000M SFP optical interface,4-port 10G SFP+ optical interface |
| SM66A-48GEF4XGEF-FB | 48-port 1000M SFP optical interface,4-port 10G SFP+ optical interface |
| SM66A-48GET4XGEF-FB | 48-port 1000M Base-T electric interface,4-port 10G SFP+ optical interface |